Fixed BOP – only 1.7 mm 145 s mixed cycles with cost multiplier of 1 are better that PCHE only cycle.

Fixed Rate – mixed cycle is always better than PCHE only cycle.

Carlson – mixed cycle is always worse than PCHE only cycle.





